**Drill Competency**

**Practical Test**

Using the 1x4 boards from the miter saw practical examination, the student will assemble

a 12” x 12” Hollywood style flat using 1-5/8” screws.

1. Assemble the four sides (stiles and rails) using pilot holes and two screws for each but joint.

1. \_\_\_\_\_\_ 2. \_\_\_\_\_\_ 3. \_\_\_\_\_\_ 4. \_\_\_\_\_\_

2. Insert the toggle between the stiles at 6” OC (on center) and use pilot holes and two screws for each joint.

 5. \_\_\_\_\_\_ 6. \_\_\_\_\_\_

All joints must be square and tight and no boards must split during assembly. Students will need to repeat the work in either instance.

Automatic failure is student fails to:

1. Follow safety guidelines
2. Dresses in a fashion inappropriate for the work assigned.