Panel Saw

Practical Competency

The student and their partner will:

1. perform a rip cut of 12” using available dimensional lumber (Luaun, hard board, plywood)
2. perform a cross cut of 6” using the same board used for the rip cut

Students are graded on:

Any element missed will need to be redone correctly.

1. Wearing safety glass
2. Appropriate clothes
3. Hearing protection
4. Proper procedures in setting up and executing a rip cut
5. Proper measurement and marking of lumber in preparation of the cross cut.
6. Proper procedures in setting up and executing a rip cut
7. Return saw to rip cut orientation
8. All cuts within 1/16”