**Power Miter Saws**

**Written Competency Test**



F

E

D

C

A

B

A

**Fill in the blank:**

**1. A. 2. B. 3. C.**

**4. D. 5. E. 6. F.**

Multiple Choice

7.\_\_\_\_\_\_The safety zone around the saw is\_\_\_\_.

A. 4” C. 8”

B. 6” D. 10”

8.\_\_\_\_\_\_Wood should be held flat against the bed and firmly againt the\_\_\_\_.

A. Blade Guard C. Fence

B. Trigger C. Miter locking handle

9.\_\_\_\_\_\_The motor should be a\_\_\_\_speed before starting a cut.

A. One Quarter C. Full

B. Half D. Doesn’t matter what

10.\_\_\_\_\_\_Be certain that the\_\_\_\_before removing the cut board.

A. blade has stopped C. sawdust is not covering the cut

B. board looks good D. pencil mark is still visible

T/F

11.\_\_\_\_\_\_A miter cut is any angled cut.

12.\_\_\_\_\_\_Safety glasses are usually required.

13.\_\_\_\_\_\_What the saw blade “takes away” is called the kerf.

14.\_\_\_\_\_\_Adjustments to the saw and/or blade can be made with the saw running.

15.\_\_\_\_\_\_Use of a jig can enable you to more accurately make multiple cuts of the same length.